



**Single Launcher Product Specification Sheet**





MANUFACTURED FROM COMPOSITE MATERIAL

PHYSICAL & OPERATIONAL

 Model Number L37-SL L40-SL

 Caliber 40mm Rifled

 Type of Action Double Action Trigger

 Safety Safety Lock

 Ammunition All Rimmed 40mm Ammo Up To 5.9” in Length

 Loading / Unloading Break Open Frame Design Allows for Quick Loading And Unloading

 Barrel 40mm 12” Long, 6 Rifling Grooves with Twist of 1”/47”

 Barrel can fit through a gun port 80mm wide by 140mm high, allowing a

 subjective sight picture and angles of fire. Barrel protrudes 12.7 cm past

 the fore-end accessory rails.

 Shoulder Stock Shoulder Stock allows the shooter a subjective sight picture while wearing

 a gas mask and riot helmet or a ballistic helmet.

 Sling Has double sided sling loops to allow carrying with a single point sling system.

 Rail NATO Standard STANAG 4694 (compatible with MIL-Std 1913 rail) This has 4 accessory rails that include a 12 o'clock mounted top rail for future optics requirements.

 Overall Length 29” With Fixed Or Open Folding Stock, 18” Closed Folding Stock

 Weight 2.6 lbs (1.18kg)

 Sight Rear Ghost Sight – Front Night Sight

SHIPPING INFORMATION

 Package Weight 4.5 lbs (2.04kg)

 Package Type Reinforced Cardboard Box

 Package Dimensions 30” x 8” x 8” (762mm x 203mm x 203mm)

 Meets NATO standard STANAG 4694 and ANSI/SAAMI Z299.5-1996

HASSLE FREE MAINTENANCE

Basic Maintenance Requirements after 100 Shots

 Remove Side Cover then Add 1 Drop of Oil to Bolt and Trigger  Standard Barrel Maintenance (As Shown Above)

